<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MK22FN512xxx12" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_12 http://mcuxpresso.nxp.com/XSD/mex_configuration_12.xsd" uuid="ee8085bc-8c28-4c9f-bf26-9ebc6d11d4c5" version="12" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_12" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MK22FN512xxx12</processor>
      <package>MK22FN512VLH12</package>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M4F" id="core0" description="M4 core"/>
      </cores>
      <description>Configuration imported from ADIS_tinyK22_Blinky</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="12.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>12.0.0</processor_version>
            <pin_labels>
               <pin_label pin_num="45" pin_signal="ADC0_SE4b/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b" label="LED_BLUE" identifier="LED_BLUE"/>
            </pin_labels>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.port" description="Pins initialization requires the PORT Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.gpio" description="Pins initialization requires the GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIOC" signal="GPIO, 2" pin_num="45" pin_signal="ADC0_SE4b/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="10.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>12.0.0</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="Bus_clock.outFreq" value="20.97152 MHz" locked="false" accuracy=""/>
                  <clock_output id="Core_clock.outFreq" value="20.97152 MHz" locked="false" accuracy=""/>
                  <clock_output id="Flash_clock.outFreq" value="10.48576 MHz" locked="false" accuracy=""/>
                  <clock_output id="FlexBus_clock.outFreq" value="10.48576 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPO_clock.outFreq" value="1 kHz" locked="false" accuracy=""/>
                  <clock_output id="MCGFFCLK.outFreq" value="32.768 kHz" locked="false" accuracy=""/>
                  <clock_output id="PLLFLLCLK.outFreq" value="20.97152 MHz" locked="false" accuracy=""/>
                  <clock_output id="System_clock.outFreq" value="20.97152 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings/>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>N/A</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="11.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>12.0.0</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="74acc050-89d1-4c54-a2cd-4d87a4233be4" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies/>
               <instances>
                  <instance name="NVIC" uuid="efec354f-7b70-430c-b629-ee71aa104f42" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="57d4dbf7-ffe2-49a1-950c-3efd0e1fbaef" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="uart_cmsis_common" uuid="7b78218d-31ba-4290-a6a1-ae1820c3e7c2" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="msg" uuid="855d17e0-ad44-40e4-9458-f02f8a82f10d" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="gpio_adapter_common" uuid="5d5e3ff2-9145-4c7d-ab47-229fafc848a8" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="97ff5def-f8e9-4b41-aa54-45b1898c920f" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_enet" uuid="d2457cac-8e6c-4e21-acf7-66dbdd91bc7c" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
            <component name="generic_can" uuid="a0eedb0b-ea00-4342-9c20-24694e234f60" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>