<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_12 http://mcuxpresso.nxp.com/XSD/mex_configuration_12.xsd" uuid="611b76b8-3631-4e76-a25d-bbc18730227b" version="12" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_12" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MK22FN512xxx12</processor>
      <package>MK22FN512VLH12</package>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="core0">
         <core name="Cortex-M4F" id="core0" description="M4 core"/>
      </cores>
      <description>Configuration imported from tinyK22_FreeRTOS</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_extended_information>false</generate_extended_information>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="13.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>13.0.1</processor_version>
            <pin_labels>
               <pin_label pin_num="45" pin_signal="ADC0_SE4b/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b" label="LED_BLUE" identifier="LED_BLUE"/>
               <pin_label pin_num="1" pin_signal="ADC1_SE4a/PTE0/CLKOUT32K/SPI1_PCS1/UART1_TX/I2C1_SDA/RTC_CLKOUT" label="TEST" identifier="TEST"/>
            </pin_labels>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>core0</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.port" description="Pins initialization requires the PORT Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.gpio" description="Pins initialization requires the GPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="core0">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIOC" signal="GPIO, 2" pin_num="45" pin_signal="ADC0_SE4b/CMP1_IN0/PTC2/SPI0_PCS2/UART1_CTS_b/FTM0_CH1/FB_AD12/I2S0_TX_FS/LPUART0_CTS_b">
                     <pin_features>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="gpio_init_state" value="true"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="11.0" enabled="true" update_project_code="true">
         <generated_project_files/>
         <clocks_profile>
            <processor_version>13.0.1</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PinSignal" resourceId="OSC.EXTAL0" description="&apos;EXTAL0&apos; (Pins tool id: OSC.EXTAL0, Clocks tool id: OSC.EXTAL0) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="OSC.EXTAL0" description="&apos;EXTAL0&apos; (Pins tool id: OSC.EXTAL0, Clocks tool id: OSC.EXTAL0) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="OSC.XTAL0" description="&apos;XTAL0&apos; (Pins tool id: OSC.XTAL0, Clocks tool id: OSC.XTAL0) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PinSignal" resourceId="OSC.XTAL0" description="&apos;XTAL0&apos; (Pins tool id: OSC.XTAL0, Clocks tool id: OSC.XTAL0) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources>
                  <clock_source id="OSC.OSC.outFreq" value="8 MHz" locked="false" enabled="true"/>
               </clock_sources>
               <clock_outputs>
                  <clock_output id="LPO_clock.outFreq" value="1 kHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="MCGMode" value="PEE" locked="false"/>
                  <setting id="MCG.FRDIV.scale" value="32" locked="false"/>
                  <setting id="MCG.IREFS.sel" value="MCG.FRDIV" locked="false"/>
                  <setting id="MCG.PLLS.sel" value="MCG.PLL" locked="false"/>
                  <setting id="MCG.PRDIV.scale" value="2" locked="false"/>
                  <setting id="MCG.VDIV.scale" value="25" locked="false"/>
                  <setting id="MCG_C2_OSC_MODE_CFG" value="ModeOscLowPower" locked="false"/>
                  <setting id="MCG_C2_RANGE0_CFG" value="High" locked="false"/>
                  <setting id="MCG_C2_RANGE0_FRDIV_CFG" value="High" locked="false"/>
                  <setting id="SIM.OUTDIV1.scale" value="5" locked="false"/>
                  <setting id="SIM.OUTDIV2.scale" value="5" locked="false"/>
                  <setting id="SIM.OUTDIV3.scale" value="10" locked="false"/>
                  <setting id="SIM.OUTDIV4.scale" value="10" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="2.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>N/A</processor_version>
         </dcdx_profile>
         <dcdx_configurations/>
      </dcdx>
      <periphs name="Peripherals" version="12.0" enabled="true" update_project_code="true">
         <dependencies>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lptmr" description="LPTMR Driver not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lptmr" description="Unsupported version of the LPTMR Driver in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.1.1</data>
               </feature>
            </dependency>
         </dependencies>
         <generated_project_files>
            <file path="board/peripherals.c" update_enabled="true"/>
            <file path="board/peripherals.h" update_enabled="true"/>
         </generated_project_files>
         <peripherals_profile>
            <processor_version>13.0.1</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="93c877a6-9f8b-4a3f-8c70-0430afa765cb" called_from_default_init="true" id_prefix="" core="core0">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="ClockOutput" resourceId="LPO_clock" description="LPO clock is inactive." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
               </dependencies>
               <instances>
                  <instance name="NVIC" uuid="84710378-f071-4dcf-b1f5-5899ccfd1cd8" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
                  <instance name="LPTMR0" uuid="f21c130f-1b13-4fbf-8185-53bae111a345" type="lptmr" type_id="lptmr_48552e76e8733b28a9c768b6d8d4fefa" mode="LPTMR_GENERAL" peripheral="LPTMR0" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="fsl_lptmr" quick_selection="QS_LPTMR_1">
                        <struct name="lptmr_config">
                           <setting name="timerMode" value="kLPTMR_TimerModeTimeCounter"/>
                           <setting name="pinSelect" value="ALT.0"/>
                           <setting name="pinPolarity" value="kLPTMR_PinPolarityActiveHigh"/>
                           <setting name="enableFreeRunning" value="false"/>
                           <setting name="bypassPrescaler" value="true"/>
                           <setting name="prescalerClockSource" value="kLPTMR_PrescalerClock_1"/>
                           <setting name="clockSource" value="ClocksTool_DefaultInit"/>
                           <setting name="value" value="kLPTMR_Prescale_Glitch_0"/>
                           <setting name="timerPeriod" value="1000000 us"/>
                        </struct>
                        <setting name="enableInterrupt" value="false"/>
                        <struct name="interrupt">
                           <setting name="IRQn" value="LPTMR0_IRQn"/>
                           <setting name="enable_interrrupt" value="enabled"/>
                           <setting name="enable_priority" value="false"/>
                           <setting name="priority" value="0"/>
                           <setting name="enable_custom_name" value="false"/>
                        </struct>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="d2de9bdf-0ffd-477f-870b-54521c2d33ea" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="msg" uuid="ebfff23e-6dd2-47aa-8f33-89c7f62e15e5" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="generic_uart" uuid="1acb5663-a9ad-4383-a5c7-dd7c48a34b20" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_can" uuid="0f842378-169a-4268-ac64-264231c6562a" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
            <component name="uart_cmsis_common" uuid="d9757538-2d94-4dcd-8424-4dc99ae79da1" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="gpio_adapter_common" uuid="0af434de-88a4-4154-b0f5-9ecf13eb8902" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_enet" uuid="1a08822c-01c1-4cea-a889-f984e70b6a60" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>